LIBRARY libnfc
VERSION 1.7

EXPORTS
  nfc_init
  nfc_exit
  nfc_register_driver
  nfc_open
  nfc_close
  nfc_abort_command
  nfc_list_devices
  nfc_idle
  nfc_initiator_init
  nfc_initiator_init_secure_element
  nfc_initiator_select_passive_target
  nfc_initiator_list_passive_targets
  nfc_initiator_poll_target
  nfc_initiator_select_dep_target
  nfc_initiator_poll_dep_target
  nfc_initiator_deselect_target
  nfc_initiator_transceive_bytes
  nfc_initiator_transceive_bits
  nfc_initiator_transceive_bytes_timed
  nfc_initiator_transceive_bits_timed
  nfc_initiator_target_is_present
  nfc_target_init
  nfc_target_send_bytes
  nfc_target_receive_bytes
  nfc_target_send_bits
  nfc_target_receive_bits
  nfc_strerror
  nfc_strerror_r
  nfc_perror
  nfc_device_get_last_error
  nfc_device_get_name
  nfc_device_get_connstring
  nfc_device_get_supported_modulation
  nfc_device_get_supported_baud_rate
  nfc_device_get_supported_baud_rate_target_mode
  nfc_device_set_property_int
  nfc_device_set_property_bool
  nfc_emulate_target
  iso14443a_crc
  iso14443a_crc_append
  iso14443b_crc
  iso14443b_crc_append
  iso14443a_locate_historical_bytes
  nfc_free
  nfc_version
  nfc_device_get_information_about
  str_nfc_modulation_type
  str_nfc_baud_rate
  str_nfc_target
  pn53x_transceive
  pn532_SAMConfiguration
  pn53x_read_register
  pn53x_write_register