EXPORTS
  ; acr122.c
  acr122_connect
  acr122_disconnect
  acr122_transceive
  acr122_firmware
  acr122_led_red

  ; libnfc.c
  nfc_configure_handle_crc
  nfc_configure_handle_parity
  nfc_configure_field
  nfc_configure_list_passive_infinite
  nfc_configure_accept_invalid_frames
  nfc_configure_accept_multiple_frames
  nfc_reader_init
  nfc_reader_transceive_7bits
  nfc_reader_transceive_bytes
  nfc_reader_transceive_bits
  nfc_reader_list_passive
  nfc_reader_mifare_cmd
  nfc_target_init
  nfc_target_receive_bytes
  nfc_target_receive_bits
  nfc_target_send_bytes
  nfc_target_send_bits
 
  ; bitutils.c
  oddparity
  oddparity_bytes
  mirror
  mirror32
  mirror64
  mirror_bytes
  swap_endian32
  swap_endian64
  append_iso14443a_crc
  print_hex
  print_hex_par
  
  